\*\*Packet switching

1.Frame relay : flexibility

2.x.25 : reliable

\*\*cell switched (faster , reliable transmission)

ATM , SMDs